Assumptions

The base system is assumed to be uncoupled (i.e., the inputs do not directly affect the outputs without affecting the states).

Mathematical Techniques

In Task 1 of this lab, the spacecraft model is implemented in Simulink. The spacecraft model is given in state space, so

(1)

(2)

where

(3)

The full state linear quadratic feedback requirement of Tasks 2 and 3 combined with the assumption that the system is uncoupled (i.e., the inputs do not directly affect the output without affecting the states) give:

(4)

Note that for the system described by the specified values in equations (3) and (4), there are 2 states, one input, and two outputs (which are just the states).

In Task 2 of this lab, a linear quadratic regulator is developed for the base spacecraft system. For a regulator, the cost function to be minimized is

(5)

and the control law takes the form

(6)

where

(7)

The Riccati Matrix, , is solved using the Matrix Riccati Equation:

(8)

where for the case of a regulator

(9)

Solving for with the base spacecraft system and

(10)

yields

(11)

This gives a value of:

(12)

For Task 3 of this lab, a linear quadratic controller with an end time of 30 seconds is developed for the base spacecraft system. For a controller, the cost function to be minimized is:

The control law, gain matrix, Riccati Matrix, and Matrix Riccati Equation are the same between controllers and regulators, and are given by equations (6) through (8), respectively. However, in the case of a controller, the derivative of the Riccati Matrix is not defined to be zero. Thus, to find the Riccati Matrix, which changes with time, the Matrix Riccati Equation is integrated backwards with initial condition:

(13)

For this system, the initial condition for integration is defined:

The values of each component of the Riccati Matrix are shown as functions of time in Figure 1. Importantly, these values were calculated at discrete time steps as there is no analytical solution to the Matrix Riccati Equation for a controller. The values are shown as continuous functions for ease of viewing. Note that because the Riccati Matrix is symmetric across the main diagonal, only three components are shown.




Figure 1. Riccati Matrix Components vs. Time

The gain matrix, is calculated real-time as the Simulink model runs according to equation (7).

The code supporting all calculations described in this section can be found in Appendix A, as well as on this GitHub Page:

<https://github.com/Connor-Lemons/Advanced-Controls-Labs/tree/main/Lab%202>

Theoretical Predictions

The goal of Task 2 was to implement a linear quadratic regulator for the base spacecraft system based on given weighting matrices. The purpose of this regulator was to keep the spacecraft within an acceptable deviation from a reference condition using acceptable amounts of control. In other words, the regulator should keep the spacecraft stable in a desired configuration (i.e., the states are within accepted values and are not changing) indefinitely. What determined the acceptable reference condition(s) and acceptable amounts of control were the weighting matrices, and .

Because a regulator functions indefinitely, it does not have an associated stop time. A consequence of this is that the Riccati Matrix, and thus the gain matrix used to determine the control, are constant with respect to time. This means that a solution to the Matrix Riccati Equation can be found analytically, and the gain matrix is easily found as a function of the Riccati Matrix.

For the regulated system, the states were expected to deviate from the initial conditions as a result of the step input being applied to the spacecraft, and then for the states to level off as the regulator worked to keep the spacecraft under control. The expected control input of the regulator was a relatively large initial value which approached a constant value as the states stopped changing.

The goal of Task 3 was to implement a linear quadratic controller for the base spacecraft system based on the same weighting matrices as were used for the linear quadratic regulator and a weighting matrix related to the final states. Unlike the regulator, the purpose of this controller was to drive the states of the spacecraft to zero in the allotted time (30 seconds). The cost function of the controller used the same and matrices as the regulator for similar purposes, but also took into account the matrix. This matrix determined how aggressively the controller attempted to reach the final states.

A controller, unlike a regulator, has a definite stop time and thus both the Riccati Matrix and the gain matrix are functions of time. Thus, the Matrix Riccati Equation cannot be solved analytically for a controller and a different technique is required. Because the end value of the Riccati Matrix is known to equal , a common way to find the Riccati Matrix for controllers is to integrate the Matrix Riccati Equation backwards using as in initial condition.

For the controlled system, the states were expected to deviate from the initial conditions as a result of the step input applied, and then for the states to be driven to zero (or close to zero, depending on the accuracy of the backwards integration) by the controller. Determining the expected control input without implementing the controller was almost impossible. The Riccati Matrix components were expected to initially remain constant, then to exhibit some change in behavior, ultimately taking on the values which would make the Riccati Matrix equal to the weighting matrix for the final states. Importantly, only three components will be plotted as the Riccati Matrix is known to be symmetric about the main diagonal.